IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
File name: "FloorConcept.ifc"
Time stamp: "2012-11-26T17:25:25"
Author: "BIM Academy"
Preprocessor: "Xbim.Ifc File Processor version 2.3.4465.26831"
Originating system: "Xbim version 2.3.4465.26831"
Authorization: "RIBA Enterprises Ltd"
Application: "NBL Element Types" version "0.1" identifier "BIM Academy Systems Converter" by Organization "BIM Academy"

People and organizations
  Person "Unknown" of Organization "Unknown"
  Owner history of Person "Unknown" of Organization "Unknown" | application "NBL Element Types" version "0.1" identifier "BIM Academy Systems Converter" by Organization "BIM Academy" | change ADDED | created 1353950725 (2012-11-26T17:25:25Z)
  Owner history of Person "Unknown" of Organization "Unknown" | application "NBL Element Types" version "0.1" identifier "BIM Academy Systems Converter" by Organization "BIM Academy" | change MODIFIED | created 1353950725 (2012-11-26T17:25:25Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Xbim"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "nbl_TritonSystems_PlatonDE25" | material: layers "nbl_TritonSystems_PlatonDE25" ("nbl_TritonSystems_PlatonDE25" 23.) | property sets: Pset_SlabCommon, nbl_General

Types
  IFCSLABTYPE "nbl_TritonSystems_PlatonDE25" | FLOOR | 1 occurrence | material: layers "nbl_TritonSystems_PlatonDE25" ("nbl_TritonSystems_PlatonDE25" 23.) | property sets: nbl_General, nbl_BuildingElementTypeCommon, xbim_MaterialFunctionAssignment | description "Platon DE25 Green Roof Drainage Membrane"

Property sets
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    Combustible = FALSE (IFCBOOLEAN)
    Compartmentation = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Reference = "" (IFCIDENTIFIER)
    SurfaceSpreadOfFlame = "" (IFCLABEL)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  nbl_General | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "" (IFCLABEL)
    BarCode = "" (IFCLABEL)
    InstallationDate = "" (IFCLABEL)
    SerialNumber = "" (IFCLABEL)
    TagNumber = "" (IFCLABEL)
    WarrantyStartDate = "" (IFCLABEL)
  nbl_General | properties | on 1 type object
    AccessibilityPerformance = "" (IFCLABEL)
    Author = "NBS" (IFCLABEL)
    BIMObjectName = "nbl_TritonSystems_PlatonDE25" (IFCLABEL)
    CodePerformance = "" (IFCLABEL)
    Colour = "Black" (IFCLABEL)
    Constituents = "" (IFCLABEL)
    Cost = "" (IFCLABEL)
    Description = "Platon DE25 Green Roof Drainage Membrane" (IFCLABEL)
    DocumentReference = "www.tritonsystems.co.uk" (IFCLABEL)
    Documentation = "www.tritonsystems.co.uk/pdf/Greenroof_DE25_DE40.pdf" (IFCLABEL)
    Features = "" (IFCLABEL)
    Finish = "" (IFCLABEL)
    Grade = "" (IFCLABEL)
    Help = "www.nationalBIMlibrary.com" (IFCLABEL)
    IssueDate = "2012-11-26" (IFCLABEL)
    LifeCyclePhase = "" (IFCLABEL)
    Manufacturer = "Triton Systems" (IFCLABEL)
    ManufacturerURL = "www.tritonsystems.co.uk" (IFCLABEL)
    Material = "HDPE (recycled)" (IFCLABEL)
    MaxCompressiveStrength = "50 jN/m2" (IFCLABEL)
    MaxPressureResistanceFilled = "715 Kn/m2" (IFCLABEL)
    MaxPressureResistanceUnfilled = "75 Kn/m2" (IFCLABEL)
    MethodOfMeasurement = "" (IFCLABEL)
    ModelLabel = "" (IFCLABEL)
    ModelReference = "Triton Platon DE25" (IFCLABEL)
    NBSDescription = "High density polyethylene studded sheets" (IFCLABEL)
    NBSReference = "45-65-50/354" (IFCLABEL)
    NominalHeight (no value)
    NominalLength (no value)
    NominalWidth (no value)
    Process = "" (IFCLABEL)
    ProductionYear = "" (IFCLABEL)
    ReferenceStandard = "" (IFCLABEL)
    ReplacementCost = "" (IFCLABEL)
    ServiceLifeDuration = "50 +" (IFCLABEL)
    ServiceLifeType = "" (IFCLABEL)
    Shape = "Rectangle" (IFCLABEL)
    Size = "1330 mm x 2220 mm" (IFCLABEL)
    SofteningTemperature = "+ 125 °C" (IFCLABEL)
    StandardHeight = "" (IFCLABEL)
    StandardLength = "1330 mm" (IFCLABEL)
    StandardThickness = "1 mm" (IFCLABEL)
    StandardWidth = "2220 mm" (IFCLABEL)
    StudHeight = "23 mm" (IFCLABEL)
    SustainabilityPerformance = "" (IFCLABEL)
    Version = "1.0" (IFCLABEL)
    WarrantyDescription = "" (IFCLABEL)
    WarrantyDurationLabour = "" (IFCLABEL)
    WarrantyDurationParts = "" (IFCLABEL)
    WarrantyGuarantorLabour = "" (IFCLABEL)
    WarrantyGuarantorParts = "" (IFCLABEL)
    WaterDrainageCapacity = "1.2 L/m per second at 2% slope" (IFCLABEL)
    WaterStorageCapacity = "6.1 L/m2" (IFCLABEL)
    Weight = "950 g/m2" (IFCLABEL)
  nbl_BuildingElementTypeCommon | properties | on 1 type object
    SystemRef1 = "NBSRef 45-65-50/354:Layers 0:0" (IFCLABEL)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)